{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Instructions","MMP","Gc vs GIIG"],"not_rendered":{"charts":2,"images":3,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Gc vs GIIG","index":2,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"MMP","index":1,"n_rows":10,"n_cols":18,"rows_kept":10,"cut":false,"hidden":false,"merged":[[4,0,4,1],[4,3,4,5],[7,17,8,17]]}
[]
[null,"UCD Mixed Mode Partition",null,null,null,null,null,null,"Cohesive Shape "]
[null,"Linear Softening","Plane Stress","Linear",null,null,null,null,2]
[null,"Dugdale","Plane Strain","BK Law"]
["Geometry and Loading",null,null,"Substrate Elastic Properties",null,null,null,null,"Cohesive  ","Failure Locus (optional)",null,"Experiment","Results"]
[null,null,null,null,null,null,null,null,"Strength",1,"m (BK Law)","(optional)"]
[null,null,null,2,null,null,null,null,null,null,1.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No. of Loops"]
["h1","h2","k","E11","E22","G12","ν12","ν23","σ","GIC","GIIC","GC","GII/G","lcz","f","GII/G (W)","GII/G (HS)"]
["mm","mm",null,"GPa","GPa","GPa",null,null,"MPa","J/m2","J/m2","J/m2",null,"mm",null,"f = 0","f = 1  ","i"]